**Pi-top3 installation guide**

Info: in this installation I am going to explain exactly how to install a pi-top3. The most important thing is to follow all the steps and read them carefully in case something goes wrong. The installation guide has been made as clear as possible and hopefully you can familiarize yourself with it, good luck!

Step 1:

What do you need:

1x pi-top3

1x sd card/micro sd card

1x persoonlijke laptop

Step 2:

All files that you have to download according to this step by step guide are going to be downloaded to your personal laptop. for using this step by step guide I would recommend putting the sd card in your personal laptop.

Step 3:

Now you are supposed to download the most recent OS (operating system) for the pi-top3. This can be done via the website: <https://www.pi-top.com/products/os>. You download the makers version of the OS (operating system).

Step 4:

Now we are going to flash, for flashing you have to use the balenaetcher program. You can download this program from this website: <https://www.balena.io/etcher/>. Once everything has been downloaded, flash the OS (operating system) file. You can do this by opening the balenaetcher program and then you select the file and finally you press flash.

Step 5:

After you have followed the installation and flash steps, take the sd card out and then put the micro sd card in the pi-top3. When you have done that, you are now going to start the installations on the pi-top3 and then you are done with all installations and you can use the pi-top3.

Step 6:

If it gets too difficult I would advise you to watch the tutorial video via this website: <https://blog.pi-top.com/2016/10/13/how-to-install-pi-topos-to-a-microsd-card>. Based on the video and this installation guide, everything should work.